1. The default IP of the machine is 192.168.8.198, and the machine supports automatic online


2. This version only supports the whole system xp-win11


3. If the output center cannot be opened, install the corresponding XP or win7 environment


4. After opening the output center, select the corresponding nozzle type and positioning system in parameters, advanced settings and nozzle type.


5. In the video and tutorial directory, check the online method of the machine, the direction of knife loading, the starting and ending points of the paper knife adjustment, and the videos of inking and ink pumping of the tx806 new machine.